MREdisplacement         Calculate the motion induced signal phase for
                        IR-MRE in biphasic material
awssigmc                Estimate noise variance for multicoil MR
                        systems
calculateQI             Obtain quantitative maps from estimated
                        ESTATICS parameters.
colMT                   MT map color scheme
estimateESTATICS        Estimate parameters in the ESTATICS model.
estimateIR              Estimate IRMRI parameters
estimateIRfluid         Estimate parameters in Inversion Recovery MRI
                        experiments model for CSF voxel
estimateIRsolid         Estimate parameters in Inversion Recovery MRI
                        experiments mixture model for non-fluid voxel
estimateIRsolidfixed    Estimate mixture parameter in Inversion
                        Recovery MRI experiments mixture model for
                        non-fluid voxel
extract.ANY-method      Methods to extract information from objects of
                        class '"MPMData"', '"ESTATICSModel"',
                        '"sESTATICSModel"', '"qMaps"', '"IRdata"',
                        '"IRfluid"' and '"IRmixed"'.
generateIRData          generate IR MRI example data
qMRI-package            Methods for Quantitative Magnetic Resonance
                        Imaging ('qMRI')
readIRData              Prepare IRMRI dataset
readMPMData             Read experimental Multi-Parameter Mapping (MPM)
                        data.
smoothESTATICS          Adaptive smoothing of ESTATICS parameters and
                        MPM data
smoothIRSolid           Smooth object generated by function
                        'estimateIRsolid'
writeESTATICS           Write maps of ESTATICS parameters in
                        standardized form as NIfTI files.
writeQI                 Write estimated maps in standardized form as
                        NIfTI files.
