Package: transfR
Type: Package
Title: Transfer of Hydrograph from Gauged to Ungauged Catchments
Version: 1.1.4
Date: 2025-03-20
Authors@R: c(
  person("Alban", "de Lavenne", role = c("aut", "cre"), comment = c(ORCID = "0000-0002-9448-3490"), email = "alban.delavenne@inrae.fr"),
  person("Christophe", "Cudennec", role = c("ths"), comment = c(ORCID = "0000-0002-1707-8926"), email = "christophe.cudennec@agrocampus-ouest.fr"),
  person("Tom", "Loree", role = c("ctb"), email = "tom.loree@agrocampus-ouest.fr"),
  person("Hervé", "Squividant", role = c("ctb"), email = "herve.squividant@agrocampus-ouest.fr")
  )
Depends: R (>= 4.1.0), stars (>= 0.4-0), sf (>= 0.8-0)
Imports: doParallel, foreach, units, glmnet, Rdpack
RdMacros: Rdpack
VignetteBuilder: knitr
Suggests: knitr, rmarkdown, elevatr, progress, whitebox
Description: A geomorphology-based hydrological modelling for transferring
    streamflow measurements from gauged to ungauged catchments. Inverse
    modelling enables to estimate net rainfall from streamflow measurements 
    following Boudhraâ et al. (2018) <doi:10.1080/02626667.2018.1425801>. 
    Resulting net rainfall is then estimated on the ungauged catchments 
    by spatial interpolation in order to finally simulate streamflow 
    following de Lavenne et al. (2016) <doi:10.1002/2016WR018716>.
License: GPL-2
URL: https://gitlab.irstea.fr/HYCAR-Hydro/transfr
BugReports: https://gitlab.irstea.fr/HYCAR-Hydro/transfr/-/issues
NeedsCompilation: yes
Encoding: UTF-8
Author: Alban de Lavenne [aut, cre] (<https://orcid.org/0000-0002-9448-3490>),
  Christophe Cudennec [ths] (<https://orcid.org/0000-0002-1707-8926>),
  Tom Loree [ctb],
  Hervé Squividant [ctb]
Maintainer: Alban de Lavenne <alban.delavenne@inrae.fr>
RoxygenNote: 7.3.2
Packaged: 2025-03-20 12:21:56 UTC; delavenne
Repository: CRAN
Date/Publication: 2025-03-20 13:10:02 UTC
Built: R 4.6.0; x86_64-w64-mingw32; 2025-12-17 04:24:29 UTC; windows
Archs: x64
