makeAP                  UAV Mission Planning tool for autonomous
                        monitoring flight tasks with respect to
                        DSM/DEM, orthophoto data retrieval.
makeTP                  Flight Track Planning tool
maxpos_on_line          applies a line to a raster and returns the
                        position of the maximum value
minBB                   Rectangle flight area around points
soloLog                 Download, reorganize and export the binary log
                        files from 3DR Solo Pixhawk controller or the
                        telemetry log files from the Solo radio control
                        unit
solo_upload             Upload MAV compliant mission File to a 3DR Solo
sp_line                 create an spatiallineobject from 2 points
sp_point                create an spatialpointobject from 1 point
tutdata_dem             DEM data set of Marburg-Biedenkopf
tutdata_dji             DJI image of a survey flight
tutdata_flightarea      Flight area planning example data
tutdata_flighttrack     GPX example data
tutdata_position        position example data
tutdata_qgc_survey      Flight area planning Qgroundcontrol planning
                        file for a 100m relative to launch survey
                        flight using a GoPro Hero4
tutdata_qgc_survey30m   Flight area planning Qgroundcontrol planning
                        file for a 30m follow terrain survey flight
                        with the DJI Air 2S
tutdata_waypoints       MAVLINK waypoint example data
vecDraw                 digitizing vector features using a simple
                        leaflet base map
